|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| VARIANT | BLOWER | PUMP | LIGHT | PUMP2 | COMBI-JET | HEAT | FILL | ZONE CONTROL PANEL | DISINFECT | RE-WASH | DRY OUT | OFF TIMER |
| ON/OFF | +/- | VARIABLE\*/\*\* | ON/OFF | +/- | INTERVAL\*/\*\*\* | VARIABLE\*/\*\* | ON/OFF | INTERVAL\*/\*\*\* | ON/OFF | INTERVAL\*/\*\*\* | ON/OFF | INTERVAL\*/\*\*\* | CONNECTION | TEMP CONT | ON/OFF | ZONE ROLLER | 6011A VOL\* | 6071A VOL\* | CHLORINE# | AUTO/BUT\*/@ | FLUSH | AUTO | AUTO/BUT\*/@ | 20 MIN |
| S01 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  | X |  |  |  |  |  |  | X |
| S02 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  |  |  |  | X |  |  | X | X |
| S03 | X | X | X | X |  | X |  | X | X |  |  |  |  | X |  |  |  |  |  |  |  |  |  | X | X |
| S04 | X | X | X | X |  | X |  |  |  |  |  |  |  | X |  |  |  | X |  |  |  |  |  |  | X |
| S05 | X | X | X | X |  | X |  |  |  |  |  |  |  | X |  |  |  |  |  |  | X |  |  | X | X |
| S06 | X | X | X | X |  | X |  | X | X |  |  | X | X |  |  |  |  |  |  |  |  |  |  | X | X |
| S07 | X | X | X | X |  | X |  | X | X | X | X |  |  |  |  |  |  |  |  |  |  |  |  | X | X |
| S08 |  |  |  | X | X |  | X | X | X |  |  |  |  | X |  |  |  |  |  |  |  |  |  |  | X |
| S09 |  |  |  | X | X |  | X | X | X |  |  |  |  | X |  |  |  |  |  |  | X |  |  |  | X |
| S10 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  |  |  |  |  |  | X |  | X |
| S11 | X | X | X | X |  | X |  |  |  |  |  |  |  | X |  |  |  |  |  |  |  |  | X |  | X |
| S12 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  | X |  |  |  |  |  |  |  | X | X |
| S13 | X | X | X | X |  | X |  |  |  |  |  |  |  |  |  | X |  |  |  |  | X |  |  | X | X |
| S14 |  |  |  | X | X |  | X | X | X |  |  |  |  |  |  | X |  |  |  |  |  |  |  |  | X |
| S15 |  |  |  | X | X |  | X | X | X |  |  |  |  |  |  | X |  |  |  |  | X |  |  |  | X |
| S16 | X | X | X | X |  | X |  |  |  |  |  |  |  | X |  | X |  |  |  |  |  |  |  | X | X |
| S17 |  |  |  | X | X |  | X | X | X |  |  |  |  | X |  | X |  |  |  |  |  |  |  |  | X |
| S18 | X | X | X | X |  | X |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | X |
| S19 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  |  |  |  | X |  |  |  | X |
| S20 |  |  |  | X | X |  | X | X | X |  |  |  |  | X |  |  |  |  |  |  | X |  |  | X |  |
| S21 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| S23 | X | X | X | X |  | X |  | X | X |  |  |  |  | X |  |  |  | X |  |  |  |  |  |  |  |
| S24 | X | X | X | X |  | X |  |  |  |  |  |  |  | X |  |  |  | X |  |  |  |  |  |  |  |
| S25 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| S26 | X | X | X | X |  | X |  | X | X |  |  |  |  |  | MS |  |  |  |  |  |  |  |  |  |  |
| S27 | X | X | X | X |  | X |  | X | X |  |  |  |  |  | SL |  |  | X |  |  |  |  |  |  |  |
| S28 | X | X | X | X |  | X |  |  |  |  |  |  |  |  | MS |  |  | X |  |  |  |  |  |  |  |
| S29 | X | X | X | X |  | X |  |  |  |  |  |  |  |  | SL |  |  |  |  |  |  |  |  |  |  |
| S30 | X | X | X | X |  | X |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | X |  |  |  |
| S31 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  | X | X |  |  |  |  |  |  |
| S32 | X | X | X | X |  | X |  |  |  |  |  |  |  |  |  |  |  | X |  |  |  |  |  |  |  |
| S33 |  |  |  | X | X |  | X | X | X |  |  |  |  |  | SL |  |  |  |  |  |  |  |  |  |  |
| S34 | X | X | X | X |  | X |  |  |  |  |  |  |  | X |  |  |  |  | X |  |  |  |  |  |  |
| S35 |  |  |  | X | X |  | X | X | X |  |  |  |  | X |  |  |  |  | X |  |  |  |  |  |  |
| S36 | X | X | X | X |  | X |  | X | X |  |  |  |  |  |  |  |  |  |  | X |  |  |  |  |  |

KOLLER CONTROL BOX – 230 8014A-S\*\* SOFTWARE VARIATIONS

\* Select this function through basic adjustment

\*\* Variation: UP/DOWN + Massage Mode

\*\*\* Interval: ON/OFF

# On fill automatic water chlorination takes place

@ Alt Button: Ability to switch ON/OFF, rewash and dry out with additional button

MS=Master

SL=Slave

|  |
| --- |
|  |
| combi-jet | This program combines the air and water system for the operation of the magic jet. |  | fill water chlori- nation | While filling the tub an automatic chlorination of the fill water takes place. |
| heating | Switch on automatically if the pump works. | rewash | Function is activated, if water was in the bath tub. Starts about 10 minutes after the tub is empty. Alter- natively it is possible tostart / stop this function at empty tub with a button. duration of the rewash: 2 minutes |
| temperature controller | Only when connected to electronic temperature indicator with adjustable function 012 3321C. Master: The heater switches on when the temper-ature falls below the set temperature. If the pump has not yet been activated, it will switch on.Slave: The heater only switches on when the temper- ature falls below the set temperature and when the pump is already operating. |
| dry out | Starts automatically, if water was in the bath tub. The dry out starts about 20 minutes after the tub is empty. Alternatively it is possible to start / stop this function with a button.duration of the dry out: 3 minutes |
| filling | Automatic filling through a button. |
| OFF-Timer | The running time limiter is activated, when the status indicator reads „Pool ready“ and the control panel registers the first pressing of the button. All whirlpool functions may be used as much, as you desire during the operating period. Upon reaching the runningtime limit, appliances switch off automatically. Should all functions be switched off during this time, the running time limiter will also reset automatically. The appliances may be immediately switched on after the automatic stop. |
| zone roller | 1-push-operation: one short push of the button changes the sequence or stops the program. A long push of the button puts the program into reference position. |
| disinfection | Starts through the button disinfection and works than automatically. The bath tub is disinfected after about 35 minutes. |
|  |